
Before you update the firmware, you must install the Kvaser drivers
and the Kvaser hardware. The procedure for this is described in a separate
document and also on our web site, www.kvaser.com.

To update the firmware:

1) Start "Update.exe".

2) These instructions are displayed.
   Click Next to continue.

3) A list of supported and currently connected Kvaser devices will now appear.
   Select the device(s) you want to upgrade.
   Click Next to continue.

4) Release notes for the selected Kvaser devices will now be available.
   Click the button(s) to open and read the individual release notes.

5) Click the Next button.

6) Click the Start Upgrade button. The programming will now start.
   Typically it takes a few seconds per device.

8) You can watch the progress in the output window. When the
   programming is done, the text "Success!" should appear in the status
   window. If not, check the output window for error messages.
   You can right click in the output window to copy its contents
   to the clipboard, if needed.

9) Close the Update program.

10) Start "Kvaser Device Guide" and check that all Kvaser devices are
    listed*.

* If you update PCIEcan or Mini PCI Express, you have to shutdown the computer.
  Not only reboot it.


===========================================================================
Those of you who are developing your own programs and want to update
the firmware from within another program - please contact us at
support@kvaser.com.
===========================================================================
