# kvrlib

Contents

- kvrlib

  - Connect to your remote device

The following sections contain sample code for inspiration on how to use Kvaser Python kvrlib.

## Connect to your remote device

    """connect_to_remote_device.py

    Use the discovery functions to scan and connect to a remote device. Our remote
    device has serial number 10545 and is already connected to the same network as our
    computer.

    """
    from canlib import kvrlib

    SERIAL_NO = 10545

    print("kvrlib version: %s" % kvrlib.getVersion())
    print("Connecting to device with serial number %s" % SERIAL_NO)

    addressList = kvrlib.kvrDiscovery.getDefaultAddresses(kvrlib.kvrAddressTypeFlag_BROADCAST)
    print("Looking for device using addresses: %s" % addressList)
    discovery = kvrlib.kvrDiscovery()
    discovery.setAddresses(addressList)
    deviceInfos = discovery.getResults()
    print("Scanning result:\n%s" % deviceInfos)
    # Connect to device with correct SERIAL_NO
    for deviceInfo in deviceInfos:
        if deviceInfo.ser_no == SERIAL_NO:
            deviceInfo.connect()
            print('\nConnecting to the following device:')
            print('---------------------------------------------')
            print(deviceInfo)
            discovery.storeDevices(deviceInfos)
            break
    discovery.close()

This results in the following:

    kvrlib version: 2070
    Connecting to device with serial number 10545
    Looking for device using addresses: 10.0.255.255:0 (IPV4_PORT)
    Scanning result:
    [
    name/hostname  : "MiMi-06348-000710" / "kv-06348-000710"
      ean/serial   : 73301-30006348 / 710
      fw           : 2.4.231
      addr/cli/AP  : 10.0.3.138 (IPV4) / 10.0.3.84 (IPV4) / - (UNKNOWN)
      availability : Availability.STORED|FOUND_BY_SCAN
      usage/access : DeviceUsage.FREE / Accessibility.PUBLIC
      pass/enc.key : yes / yes,
    name/hostname  : "TestClient1-2-DUT-01" / "swtdut01"
      ean/serial   : 73301-30006713 / 10545
      fw           : 3.4.822
      addr/cli/AP  : 10.0.3.54 (IPV4) / 10.0.3.98 (IPV4) / - (UNKNOWN)
      availability : Availability.STORED|FOUND_BY_SCAN
      usage/access : DeviceUsage.REMOTE / Accessibility.PUBLIC
      pass/enc.key : yes / yes]

    Connecting to the following device:
    ---------------------------------------------

    name/hostname  : "TestClient1-2-DUT-01" / "swtdut01"
      ean/serial   : 73301-30006713 / 10545
      fw           : 3.4.822
      addr/cli/AP  : 10.0.3.54 (IPV4) / 10.0.3.98 (IPV4) / - (UNKNOWN)
      availability : Availability.STORED|FOUND_BY_SCAN
      usage/access : DeviceUsage.REMOTE / Accessibility.PUBLIC
      pass/enc.key : yes / yes