# Convert a .kme50 file to plain ASCII

    """convert_kme_asc.py -- Convert a .kme50 logfile into plain ASCII

    This example script uses canlib.kvlclib to convert a logfile from .kme50 format
    into plain ASCII.

    """
    import argparse
    from pathlib import Path

    from canlib import kvlclib

    def try_set_propery(cnv, property, value=None):
        # Check if the format supports the given property
        if cnv.format.isPropertySupported(property):
            # If a value is specified, set the property to this value
            if value is not None:
                cnv.setProperty(property, value)

            # Get the property's default value
            default = cnv.format.getPropertyDefault(property)
            print(f'  {property} is supported (Default: {default})')

            # Get the property's current value
            value = cnv.getProperty(property)
            print(f'    Current value: {value}')
        else:
            print(f'  {property} is not supported')

    def convert_events(cnv):
        # Get estimated number of remaining events in the input file. This
        # can be useful for displaying progress during conversion.
        total = cnv.eventCount()
        print(f"Converting about {total} events...")
        while True:
            try:
                # Convert events from input file one by one until EOF
                # is reached
                cnv.convertEvent()
                if cnv.isOutputFilenameNew():
                    print(f"New output filename: '{cnv.getOutputFilename()}'")
                    print(f"About {cnv.eventCount()} events left...")
            except kvlclib.KvlcEndOfFile:
                if cnv.isOverrunActive():
                    print("NOTE! The extracted data contained overrun.")
                    cnv.resetOverrunActive()
                if cnv.isDataTruncated():
                    print("NOTE! The extracted data was truncated.")
                    cnv.resetStatusTruncated()
                break

    if __name__ == '__main__':
        parser = argparse.ArgumentParser(description="Convert a .kme50 logfile into plain ASCII.")
        parser.add_argument(
            'filename', metavar='LOGFILE.KME50', help=("The filename of the .kme50 logfile.")
        )
        args = parser.parse_args()
        in_file = Path(args.filename)

        # set up formats
        out_fmt = kvlclib.WriterFormat(kvlclib.FileFormat.PLAIN_ASC)
        in_fmt = kvlclib.ReaderFormat(kvlclib.FileFormat.KME50)

        # set resulting output file name taking advantage of the extension
        # defined in the format.
        out_file = in_file.with_suffix('.' + out_fmt.extension)
        print(f"Output filename is '{out_file}'")

        # create converter
        cnv = kvlclib.Converter(out_file, out_fmt)

        # Set input file and format
        cnv.setInputFile(in_file, kvlclib.FileFormat.KME50)

        # split output files into max 100 MB files
        # The name of the resulting files will now end in '-partX.txt',
        # thus the first file will be named logfile-part0.txt, assuming we use
        # logfile.kme50 as input file name.
        try_set_propery(cnv, kvlclib.Property.SIZE_LIMIT, 100)

        # allow output file to overwrite existing files
        try_set_propery(cnv, kvlclib.Property.OVERWRITE, 1)

        # we are only interested in the first channel
        cnv.setProperty(kvlclib.Property.CHANNEL_MASK, 1)

        # add nice header to the output file
        try_set_propery(cnv, kvlclib.Property.WRITE_HEADER, 1)

        # we are converting CAN traffic with max 8 bytes, so we can minimize
        # the width of the data output to 8 bytes
        try_set_propery(cnv, kvlclib.Property.LIMIT_DATA_BYTES, 8)

        convert_events(cnv)

        # force flush result to disk
        cnv.flush()

## Description

We have created a wrapper function `try_set_propery` that will examine the property we are trying to set, and ignore the setting if the current format used does not support the property. While converting events in the `convert_events` function, we also inform the user if any overruns or data truncation was detected.

## Sample Output

    C:\example>python convert_kme_asc.py gensig.kme50
    Output filename is 'C:\example\gensig.txt'
      Property.SIZE_LIMIT is supported (Default: 0)
        Current value: 100
      Property.OVERWRITE is supported (Default: 0)
        Current value: 1
      Property.WRITE_HEADER is supported (Default: 0)
        Current value: 1
      Property.LIMIT_DATA_BYTES is supported (Default: 64)
        Current value: 8
    Converting about 310 events...
    New output filename: 'C:\example\gensig-part0.txt
    About 309 events left...