# Write a Configuration to a Memorator

    """write_memo_config.py -- Write a configuration to a memorator

    This example script uses canlib.kvamemolibxml and canlib.kvmlib to load a
    configuration file in .xml format, validate it, and then write it to a
    connected Memorator.

    It requires a configuration xml file and a connected Memorator device.

    """
    import argparse

    from canlib import kvamemolibxml
    from canlib import kvmlib

    def write_config(filename, channel_number):
        # Read in the XML configuration file
        config = kvamemolibxml.load_xml_file(filename)

        # Validate the XML configuration
        errors, warnings = config.validate()

        if errors or warnings:
            raise Exception("Errors or warnings found! Check validate_memo_config example.")

        # Open the device and write the configuration
        with kvmlib.openDevice(channel_number) as memo:
            memo.write_config(config.lif)

    if __name__ == '__main__':
        parser = argparse.ArgumentParser(
            description="Write a configuration to a Memorator.")
        parser.add_argument('filename', default='logall.xml', nargs='?', help=(
            "The filename of the configuration."))
        parser.add_argument('channel', type=int, default=0, nargs='?', help=(
            "The channel number of the device the configuration should be written to."))
        args = parser.parse_args()

        write_config(args.filename, args.channel_number)