# Source code for canlib.canlib.wrapper

    import ctypes as ct
    import struct
    import sys
    import logging

    from .. import dllLoader
    from .. import deprecation
    from .. import BetaVersionNumber, VersionNumber
    from .dll import CanlibDll
    from .enums import VersionEx
    from . import constants as const

    _ct_dll = dllLoader.load_dll(win_name='canlib32.dll',
                                 linux_name='libcanlib.so')
    dll = CanlibDll(_ct_dll)
    dll.canInitializeLibrary()

    class bitrateSetting(object):
        """
        Class that holds bitrate setting.

        Attributes:
            freq: Bitrate in bit/s.
            tseg1: Number of quanta from (but not including) the Sync Segment to
                the sampling point.
            tseg2: Number of quanta from the sampling point to the end of the bit.
            sjw: The Synchronization Jump Width, can be 1,2,3, or 4.
            nosamp: The number of sampling points, only 1 is supported.
            syncMode: Unsupported and ignored.
        """

        def __init__(self, freq=1000000, tseg1=4, tseg2=3, sjw=1, nosamp=1,
                     syncMode=0):
            self.freq = freq
            self.tseg1 = tseg1
            self.tseg2 = tseg2
            self.sjw = sjw
            self.nosamp = nosamp
            self.syncMode = syncMode

        def __eq__(self, other):
            if self.freq != other.freq:
                return False
            if self.tseg1 != other.tseg1:
                return False
            if self.tseg2 != other.tseg2:
                return False
            if self.sjw != other.sjw:
                return False
            if self.nosamp != other.nosamp:
                return False
            if self.syncMode != other.syncMode:
                return False
            return True

        def __ne__(self, other):
            return not self.__eq__(other)

        def __str__(self):
            txt = "freq    : %8d\n" % self.freq
            txt += "tseg1   : %8d\n" % self.tseg1
            txt += "tseg2   : %8d\n" % self.tseg2
            txt += "sjw     : %8d\n" % self.sjw
            txt += "nosamp  : %8d\n" % self.nosamp
            txt += "syncMode: %8d\n" % self.syncMode
            return txt

    class CANLib(object):
        """Deprecated wrapper class for the Kvaser CANlib.

        .. deprecated:: 1.5

        All functionality of this class has been moved to the canlib module itself::

          # deprecated
          from canlib import canlib
          cl = canlib.CANLib()  # or canlib.canlib()
          cl.functionName()

          # use this instead
          from canlib import canlib
          canlib.functionName()

        """
        dll = dll

        def __init__(self):
            deprecation.manual_warn(
                "Creating CANLib objects is deprecated, "
                "all functionality has been moved to the canlib module itself.")
            # since=1.5
            self._module = sys.modules[__name__]

        def __getattr__(self, name):
            try:
                return getattr(self._module, name)
            except AttributeError:
                raise AttributeError("{t} object has no attribute {n}".format(
                    t=str(type(self)), n=name))

        def openChannel(self, channel, flags=0):
            from .channel import openChannel
            return openChannel(channel, flags)

    def getErrorText(error_code):
        """Return error text for supplied error_code"""
        msg = ct.create_string_buffer(80)
        dll.canGetErrorText(error_code, msg, ct.sizeof(msg))
        return msg.value.decode()

    @deprecation.deprecated.favour('dllversion')
    def getVersion():
        """Get the CANlib DLL version number as a `str`

        .. deprecated:: 1.5
           Use `dllversion` instead.

        """
        return str(dllversion())

    def _version_number(v, beta):
        """Return `VersionNumber` or `BetaVersionNumber` of v"""
        # assuming byte order 'little':
        if beta:
            version = BetaVersionNumber(major=v >> 8, minor=v & 0xff)
        else:
            version = VersionNumber(major=v >> 8, minor=v & 0xff)
        return version

    def dllversion():
        """Get the CANlib DLL version number

        Args:
            None

        Returns a `BetaVersionNumber` if the CANlib DLL is marked as beta
        (preview), otherwise returns `VersionNumber`.

        .. versionchanged:: 1.6

        """
        try:
            v = dll.canGetVersionEx(VersionEx.VERSION)
        except NotImplementedError:
            # Backward compatibility with CANlib v5.22
            v = dll.canGetVersion()
            return _version_number(v, beta=False)
        beta = dll.canGetVersionEx(VersionEx.BETA)
        return _version_number(v, beta)

    def prodversion():
        """Get the CANlib Product version number

        Args:
            driver (bool): If `True` driver will be asked, otherwise DLL will be asked.

        Returns a `BetaVersionNumber` if the CANlib driver/DLL is marked as beta
        (preview), otherwise returns `VersionNumber`.

        .. versionadded:: 1.6

        """
        v = dll.canGetVersionEx(VersionEx.PRODVER)
        beta = dll.canGetVersionEx(VersionEx.BETA)
        return _version_number(v, beta)

    def getNumberOfChannels(driver=False):
        """Get number of available CAN channels.

        Returns the number of available CAN channels in the computer. The
        virtual channels are included in this number.

        Args:
            None

        Returns:
            chanCount (int): Number of available CAN channels

        """
        chanCount = ct.c_int()
        dll.canGetNumberOfChannels(chanCount)
        return chanCount.value

    @deprecation.deprecated.favour("ChannelData(channel).channel_flags")
    def getChannelData_Channel_Flags(channel):
        """Get channel status flags

        .. deprecated:: 1.5
           Use `ChannelData` and their ``channel_flags`` attribute instead.

        Returns a :py:class:`ChannelData_Channel_Flags` object holding
        information about the channel.

        Note: Currently not implemented!

        """
        buf = ct.c_uint32()
        dll.canGetChannelData(
            channel,
            const.canCHANNELDATA_CHANNEL_FLAGS,
            ct.byref(buf),
            ct.sizeof(buf),
        )
        flags = ChannelData_Channel_Flags()
        flags.asbyte = buf.value
        return flags

    @deprecation.deprecated.favour("ChannelData(channel).device_name")
    def getChannelData_Name(channel):
        """Get the product name.

        .. deprecated:: 1.5
           Use `ChannelData` and their ``device_name`` attribute instead.

        Retrieves the product name of the device connected to channel. The name
        is returned as a string.

        Args:
            channel (int): The channel you are interested in

        Returns:
            product_name (string): The product name

        """
        name = ct.create_string_buffer(80)
        dll.canGetChannelData(
            channel,
            const.canCHANNELDATA_DEVDESCR_ASCII,
            ct.byref(name),
            ct.sizeof(name),
        )
        buf_type = ct.c_uint * 1
        buf = buf_type()
        dll.canGetChannelData(
            channel,
            const.canCHANNELDATA_CHAN_NO_ON_CARD,
            ct.byref(buf),
            ct.sizeof(buf),
        )
        return "%s (channel %d)" % (name.value.decode(), buf[0])

    @deprecation.deprecated.favour("ChannelData(channel).custom_name")
    def getChannelData_Cust_Name(channel):
        """Get the customized channel name.

        .. deprecated:: 1.5
           Use `ChannelData` and their ``custom_name`` attribute instead.

        Retrieves the customized device channel name of the device connected to
        channel. The name is returned as a string.

        Args:
            channel (int): The channel you are interested in

        Returns:
            custom_name (string): The customized device channel name

        """

        name = ct.create_string_buffer(40)
        dll.canGetChannelData(
            channel,
            const.canCHANNELDATA_CUST_CHANNEL_NAME,
            ct.byref(name),
            ct.sizeof(name),
        )
        return "%s" % (name.value.decode())

    @deprecation.deprecated.favour("ChannelData(channel).chan_no_on_card")
    def getChannelData_Chan_No_On_Card(channel):
        """Get the channel number on the card.

        .. deprecated:: 1.5
           Use `ChannelData` and their ``chan_no_on_card`` attribute instead.

        Retrieves the channel number, as numbered locally on the card, device
        connected to channel.

        Args:
            channel (int): The channel you are interested in

        Returns:
            number (int): The local channel number

        """
        number = ct.c_ulong()
        dll.canGetChannelData(
            channel,
            const.canCHANNELDATA_CHAN_NO_ON_CARD,
            ct.byref(number),
            ct.sizeof(number),
        )
        buf_type = ct.c_uint * 1
        buf = buf_type()
        dll.canGetChannelData(
            channel,
            const.canCHANNELDATA_CHAN_NO_ON_CARD,
            ct.byref(buf),
            ct.sizeof(buf),
        )
        return number.value

    @deprecation.deprecated.favour("ChannelData(channel).card_number")
    def getChannelData_CardNumber(channel):
        """Get the card number

        .. deprecated:: 1.5
           Use `ChannelData` and their ``card_number`` attribute instead.

        Retrieves the card's number in the computer. Each card type is numbered
        separately. For example, the first PCIEcan card in a machine will have
        number 0, the second PCIEcan number 1, etc.

        Args:
            channel (int): The channel you are interested in

        Returns:
            card_number (int): The device's card number

        """
        buf_type = ct.c_ulong
        buf = buf_type()
        dll.canGetChannelData(
            channel,
            const.canCHANNELDATA_CARD_NUMBER,
            ct.byref(buf),
            ct.sizeof(buf),
        )
        return buf.value

    @deprecation.deprecated.favour("ChannelData(channel).card_upc_no")
    def getChannelData_EAN(channel):
        """Get EAN code

        .. deprecated:: 1.5
           Use `ChannelData` and their ``card_upc_no`` attribute instead.

        Retrieves the EAN number for the device connected to channel. If there
        is no EAN number, "00-00000-00000-0" will be returned.

        Args:
            channel (int): The channel you are interested in

        Returns:
            ean (str): The device's EAN number

        """
        buf_type = ct.c_uint32 * 2
        buf = buf_type()
        dll.canGetChannelData(
            channel,
            const.canCHANNELDATA_CARD_UPC_NO,
            ct.byref(buf),
            ct.sizeof(buf),
        )
        (ean_lo, ean_hi) = struct.unpack('II', buf)
        return "%02x-%05x-%05x-%x" % (ean_hi >> 12,
                                      ((ean_hi & 0xfff) << 8) | (ean_lo >> 24),
                                      (ean_lo >> 4) & 0xfffff, ean_lo & 0xf)

    @deprecation.deprecated
    def getChannelData_EAN_short(channel):
        """Get short EAN code

        .. deprecated:: 1.5
           Use `ChannelData` and their ``.card_upc_no.product()`` instead.

        Retrieves the short EAN number, aka product number, for the device
        connected to channel. If there is no EAN number, "00000-0" will be
        returned.

        Args:
            channel (int): The channel you are interested in

        Returns:
            ean (str): The device's shortened EAN number

        """
        buf_type = ct.c_uint32 * 2
        buf = buf_type()
        dll.canGetChannelData(
            channel,
            const.canCHANNELDATA_CARD_UPC_NO,
            ct.byref(buf),
            ct.sizeof(buf),
        )
        (ean_lo, ean_hi) = struct.unpack('II', buf)
        return "%04x-%x" % ((ean_lo >> 4) & 0xffff, ean_lo & 0xf)

    @deprecation.deprecated.favour("ChannelData(channel).card_serial_no")
    def getChannelData_Serial(channel):
        """Get device serial number

        .. deprecated:: 1.5
           Use `ChannelData` and their ``card_serial_no`` attribute instead.

        Retrieves the serial number for the device connected to channel. If the
        device does not have a serial number, 0 is returned.

        Args:
            channel (int): The channel you are interested in

        Returns:
            serial (int): The device serial number

        """
        buf_type = ct.c_uint32 * 2
        buf = buf_type()
        dll.canGetChannelData(
            channel,
            const.canCHANNELDATA_CARD_SERIAL_NO,
            ct.byref(buf),
            ct.sizeof(buf),
        )
        (serial_lo, serial_hi) = struct.unpack('II', buf)
        # serial_hi is always 0
        return serial_lo

    @deprecation.deprecated.favour("ChannelData(channel).driver_name")
    def getChannelData_DriverName(channel):
        """Get device driver name

        .. deprecated:: 1.5
           Use `ChannelData` and their ``driver_name`` attribute instead.

        Retrieves the name of the device driver (e.g. "kcany") for the device
        connected to channel. The device driver names have no special meanings
        and may change from a release to another.

        Args:
            channel (int): The channel you are interested in

        Returns:
            driver_name (str): The device driver name

        """
        name = ct.create_string_buffer(80)
        dll.canGetChannelData(
            channel,
            const.canCHANNELDATA_DRIVER_NAME,
            ct.byref(name),
            ct.sizeof(name),
        )
        return name.value.decode()

    @deprecation.deprecated.favour("ChannelData(channel).card_firmware_rev")
    def getChannelData_Firmware(channel):
        """Get device firmware version

        .. deprecated:: 1.5
           Use `ChannelData` and their ``card_firmware_rev`` attribute instead.

        Retrieves the firmvare version numbers for the device connected to
        channel.

        Args:
            channel (int): The channel you are interested in

        Returns:
            (fw_major, fw_minor, fw_build): The version number

        """
        buf_type = ct.c_ushort * 4
        buf = buf_type()
        dll.canGetChannelData(
            channel,
            const.canCHANNELDATA_CARD_FIRMWARE_REV,
            ct.byref(buf),
            ct.sizeof(buf),
        )
        (build, release, minor, major) = struct.unpack('HHHH', buf)
        return (major, minor, build)

    def translateBaud(freq):
        """Translate bitrate constant

        This function translates the canBITRATE_xxx constants to their
        corresponding bus parameter values.

        Args:
            freq: Any of the predefined constants canBITRATE_xxx

        Returns:
            A bitrateSetting object containing the actual values of
                frequency, tseg1, tseg2 etc.

        """
        freq_p = ct.c_long(freq)
        tseg1_p = ct.c_uint()
        tseg2_p = ct.c_uint()
        sjw_p = ct.c_uint()
        nosamp_p = ct.c_uint()
        syncMode_p = ct.c_uint()
        dll.canTranslateBaud(
            ct.byref(freq_p),
            ct.byref(tseg1_p),
            ct.byref(tseg2_p),
            ct.byref(sjw_p),
            ct.byref(nosamp_p),
            ct.byref(syncMode_p),
        )
        rateSetting = bitrateSetting(
            freq=freq_p.value,
            tseg1=tseg1_p.value,
            tseg2=tseg2_p.value,
            sjw=sjw_p.value,
            nosamp=nosamp_p.value,
            syncMode=syncMode_p.value,
        )
        return rateSetting

    def unloadLibrary():
        """Unload CANlib

        Unload canlib and release all internal handles.

        Warning:

            Calling `unloadLibrary` invalidates every canlib-object. Use at your
            own risk.

        """
        try:
            dll.canUnloadLibrary()
        except AttributeError as e:
            logging.debug(str(e) + ' (Not implemented in Linux)')

    def initializeLibrary():
        """Initialize CANlib library

        Note:

            This initializes the driver and must be called before any other
            function in the CANlib DLL is used. This is handled in most cases by
            the Python wrapper but if you want to trigger a re-enumeration of
            connected devices, call this function.

        Any errors encountered during library initialization will be "silent"
        and an appropriate error code will be returned later on when an API
        call that requires initialization is called.

        """
        dll.canInitializeLibrary()

    def reinitializeLibrary():
        """Reinitializes the CANlib driver.

        Convenience function that calls `unloadLibrary` and `initializeLibrary`
        in succession.

        """
        unloadLibrary()
        dll.canInitializeLibrary()

    class ChannelData_Channel_Flags_bits(ct.LittleEndianStructure):
        """Access flags of :py:class:`ChannelData_Channel_Flags`

        .. deprecated:: 1.5

        Gives access to individual parts in :py:class:`ChannelData_Channel_Flags`
        as flags.
        """
        _fields_ = [
            ("is_exclusive", ct.c_uint32, 1),
            ("is_open", ct.c_uint32, 1),
            ("is_canfd", ct.c_uint32, 1),
        ]

    class ChannelData_Channel_Flags(ct.Union):
        """Holds data from :py:meth:`canlib.getChannelData_Channel_Flags()`

        .. deprecated:: 1.5

        Data in this object may be accessed as an c_uint32 using `object.asbyte`,
        or as indivisual flags using the class
        :py:class:`ChannelData_Channel_Flags_bits`.

        """
        _fields_ = [("b", ChannelData_Channel_Flags_bits),
                    ("asbyte", ct.c_uint32)]