# Source code for canlib.kvmlib.enums

    from ..cenum import CEnum

    class Error(CEnum):
        FAIL = -1
        PARAM = -3
        LOGFILEOPEN = -8
        NOSTARTTIME = -9
        NOLOGMSG = -10
        LOGFILEWRITE = -11
        EOF = -12
        NO_DISK = -13
        LOGFILEREAD = -14
        QUEUE_FULL = -20
        CRC_ERROR = -21
        SECTOR_ERASED = -22
        FILE_ERROR = -23
        DISK_ERROR = -24
        DISKFULL_DIR = -25
        DISKFULL_DATA = -26
        SEQ_ERROR = -27
        FILE_SYSTEM_CORRUPT = -28
        UNSUPPORTED_VERSION = -29
        NOT_IMPLEMENTED = -30
        FATAL_ERROR = -31
        ILLEGAL_REQUEST = -32
        FILE_NOT_FOUND = -33
        NOT_FORMATTED = -34
        WRONG_DISK_TYPE = -35
        TIMEOUT = -36
        DEVICE_COMM_ERROR = -37
        OCCUPIED = -38
        USER_CANCEL = -39
        FIRMWARE = -40
        CONFIG_ERROR = -41
        WRITE_PROT = -42

    class Device(CEnum):
        """kvmDEVICE_xxx

        Device type, used to connect to a Memorator device.

        """
        MHYDRA = 0
        MHYDRA_EXT = 1

    class FileType(CEnum):
        """kvmFILE_xxx

        KME file type, a binary file format representing log data.

        """
        KME24 = 0  # Deprecated format, use KME40
        KME25 = 1  # Deprecated format, use KME40
        KME40 = 2
        KME50 = 3

    class LoggerDataFormat(CEnum):
        """kvmLDF_MAJOR_xxx

        Logged data format (LDF) version.

        """
        MAJOR_CAN = 3  # Used in Kvaser Memorator (2nd generation)
        MAJOR_CAN64 = 5  # Used in Kvaser Memorator (2nd generation) with
        # extended data capabilities.

    class SoftwareInfoItem(CEnum):
        """kvm_SWINFO_xxx

        Different types of version information that can be extracted using
        kvmDeviceGetSoftwareInfo().

        """
        KVMLIB = 1
        DRIVER = 2
        FIRMWARE = 3
        CONFIG_VERSION_NEEDED = 5