# Source code for canlib.kvlclib.enums

    from ..cenum import CEnum, CFlag

    class Error(CEnum):
        FAIL = -1   # Generic error.
        PARAM = -2   # Error in supplied parameters.
        EOF = -3   # End of input file reached.
        NOT_IMPLEMENTED = -4   # Not implemented.
        FILE_ERROR = -5   # File I/O error.
        FILE_EXISTS = -6   # Output file already exists.
        INTERNAL_ERROR = -7   # Unhandled internal error.
        NULL_POINTER = -8   # Unexpected null pointer.
        FILE_TOO_LARGE = -10   # File size too large for specified format.
        TYPE_MISMATCH = -11   # Supplied parameter has incorrect type.
        NO_FREE_HANDLES = -12   # Too many open KvlcHandle handles.
        NO_INPUT_SELECTED = -13  # Missing call to kvlcSetInputFile or kvlcFeedSelectFormat.
        CONVERTING = -14   # Call failed since conversion is running.
        BUFFER_SIZE = -15   # Supplied buffer too small to hold the result.
        INVALID_LOG_EVENT = -30   # Event is unknown to converter.
        NO_TIME_REFERENCE = -31   # Required timestamp missing.
        TIME_DECREASING = -32   # Decreasing time between files.
        MIXED_ENDIANESS = -33   # Wrong data type in MDF.

    class FileFormat(CEnum):
        """FILE_FORMAT_xxx

        Format used for input and output, used in kvlcSetInputFile(),
        kvlcFeedSelectFormat().

        Note:
            Not all formats are valid as both output and input format.

        """
        INVALID = 0  # Invalid file format
        KME24 = 1    # Input and output file format.
        KME25 = 2    # Input and output file format.
        VECTOR_ASC = 3    # Output file format.
        CSV = 4    # Output file format.
        PLAIN_ASC = 5    # Output file format.
        MEMO_LOG = 6    # Input (internal device logfile format).
        KME40 = 7    # Input and output file format.
        VECTOR_BLF = 8    # Output file format.
        KME50 = 9    # Input and output file format.
        CSV_SIGNAL = 100    # Output file format.
        MDF = 101    # Output file format.
        MATLAB = 102    # Output file format.
        J1587 = 103    # Output file format.
        J1587_ALT = 104    # Obsolete.
        FAMOS = 105    # Output file format.
        MDF_SIGNAL = 106    # Output file format.
        MDF_4X = 107    # Output file format.
        MDF_4X_SIGNAL = 108    # Output file format.
        XCP = 200    # Output file format.
        FAMOS_XCP = 201    # Output file format.
        DEBUG = 1000    # Reserved for debug.

    class ChannelMask(CFlag):
        """Masking channels

        The `ChannelMask` is used in `Converter.addDatabaseFile` to indicate which channels to use.

        """
        ONE = 0x01
        TWO = 0x02
        THREE = 0x04
        FOUR = 0x08
        FIVE = 0x10