# Source code for canlib.canlib.dll

    import ctypes as ct
    import sys

    from .. import dllLoader
    from .exceptions import can_error

    _no_errcheck = dllLoader.no_errcheck

    if sys.platform.startswith('win'):
        KVCALLBACK_T = ct.WINFUNCTYPE(None, ct.c_int, ct.c_void_p, ct.c_uint)
    else:
        KVCALLBACK_T = ct.CFUNCTYPE(None, ct.c_int, ct.c_void_p, ct.c_uint)

    class CanlibDll(dllLoader.MyDll):
        function_prototypes = {
            'canAccept': [[ct.c_int, ct.c_long, ct.c_uint]],
            'canBusOff': [[ct.c_int]],
            'canBusOn': [[ct.c_int]],
            'canClose': [[ct.c_int]],
            'canGetBusParams': [[ct.c_int, ct.POINTER(ct.c_long), ct.POINTER(ct.c_uint), ct.POINTER(ct.c_uint), ct.POINTER(ct.c_uint), ct.POINTER(ct.c_uint), ct.POINTER(ct.c_uint)]],
            'canGetBusParamsFd': [[ct.c_int, ct.POINTER(ct.c_long), ct.POINTER(ct.c_uint), ct.POINTER(ct.c_uint), ct.POINTER(ct.c_uint)]],
            'canGetChannelData': [[ct.c_int, ct.c_int, ct.c_void_p, ct.c_size_t]],
            'canGetErrorText': [[ct.c_int, ct.c_char_p, ct.c_uint]],
            'canGetNumberOfChannels': [[ct.POINTER(ct.c_int)]],
            'canGetVersion': [[], ct.c_short, _no_errcheck],  # Never fails (supposedly)
            'canGetVersionEx': [[ct.c_uint], ct.c_uint, _no_errcheck],  # Never fails
            'canInitializeLibrary': [[], None, _no_errcheck],  # Returns void, no errcheck function
            'canIoCtl': [[ct.c_int, ct.c_uint, ct.c_void_p, ct.c_uint]],
            'canOpenChannel': [[ct.c_int, ct.c_int]],
            'canReadSpecificSkip': [[ct.c_int, ct.c_long, ct.c_void_p, ct.POINTER(ct.c_uint), ct.POINTER(ct.c_uint), ct.POINTER(ct.c_ulong)]],
            'canReadStatus': [[ct.c_int, ct.POINTER(ct.c_ulong)]],
            'canReadSyncSpecific': [[ct.c_int, ct.c_long, ct.c_ulong]],
            'canReadWait': [[ct.c_int, ct.POINTER(ct.c_long), ct.c_void_p, ct.POINTER(ct.c_uint), ct.POINTER(ct.c_uint), ct.POINTER(ct.c_ulong), ct.c_ulong]],
            'canRequestChipStatus': [[ct.c_int]],
            'canSetAcceptanceFilter': [[ct.c_int, ct.c_uint, ct.c_uint, ct.c_int]],
            'canSetBusOutputControl': [[ct.c_int, ct.c_ulong]],
            'canSetBusParams': [[ct.c_int, ct.c_long, ct.c_uint, ct.c_uint, ct.c_uint, ct.c_uint, ct.c_uint]],
            'canSetBusParamsFd': [[ct.c_int, ct.c_long, ct.c_uint, ct.c_uint, ct.c_uint]],
            'canTranslateBaud': [[ct.POINTER(ct.c_long), ct.POINTER(ct.c_uint), ct.POINTER(ct.c_uint), ct.POINTER(ct.c_uint), ct.POINTER(ct.c_uint), ct.POINTER(ct.c_uint)]],
            'canUnloadLibrary': [[]],
            'canWrite': [[ct.c_int, ct.c_long, ct.c_void_p, ct.c_uint, ct.c_uint]],
            'canWriteSync': [[ct.c_int, ct.c_long]],
            'canWriteWait': [[ct.c_int, ct.c_long, ct.c_void_p, ct.c_uint, ct.c_uint, ct.c_ulong]],
            'kvDeviceGetMode': [[ct.c_int, ct.POINTER(ct.c_int)]],
            'kvDeviceSetMode': [[ct.c_int, ct.c_int]],
            'kvFileCopyFromDevice': [[ct.c_int, ct.c_char_p, ct.c_char_p]],
            'kvFileCopyToDevice': [[ct.c_int, ct.c_char_p, ct.c_char_p]],
            'kvFileDelete': [[ct.c_int, ct.c_char_p]],
            'kvFileGetCount': [[ct.c_int, ct.POINTER(ct.c_int)]],
            'kvFileGetName': [[ct.c_int, ct.c_int, ct.c_char_p, ct.c_int]],
            'kvFlashLeds': [[ct.c_int, ct.c_int, ct.c_int]],
            'kvIoConfirmConfig': [[ct.c_int]],
            'kvIoGetNumberOfPins': [[ct.c_int, ct.POINTER(ct.c_uint)]],
            'kvIoPinGetAnalog': [[ct.c_int, ct.c_uint, ct.POINTER(ct.c_float)]],
            'kvIoPinGetDigital': [[ct.c_int, ct.c_uint, ct.POINTER(ct.c_uint)]],
            'kvIoPinGetInfo': [[ct.c_int, ct.c_uint, ct.c_int, ct.c_void_p, ct.c_uint]],
            'kvIoPinGetOutputAnalog': [[ct.c_int, ct.c_uint, ct.POINTER(ct.c_float)]],
            'kvIoPinGetOutputDigital': [[ct.c_int, ct.c_uint, ct.POINTER(ct.c_uint)]],
            'kvIoPinGetOutputRelay': [[ct.c_int, ct.c_uint, ct.POINTER(ct.c_uint)]],
            'kvIoPinSetAnalog': [[ct.c_int, ct.c_uint, ct.c_float]],
            'kvIoPinSetDigital': [[ct.c_int, ct.c_uint, ct.c_uint]],
            'kvIoPinSetInfo': [[ct.c_int, ct.c_uint, ct.c_int, ct.c_void_p, ct.c_uint]],
            'kvIoPinSetRelay': [[ct.c_int, ct.c_uint, ct.c_uint]],
            'kvReadDeviceCustomerData': [[ct.c_int, ct.c_int, ct.c_int, ct.c_void_p, ct.c_size_t]],
            'kvReadTimer': [[ct.c_int, ct.POINTER(ct.c_int)]],
            'kvScriptEnvvarClose': [[ct.c_int64]],
            'kvScriptEnvvarGetData': [[ct.c_int64, ct.c_void_p, ct.c_int, ct.c_int]],
            'kvScriptEnvvarGetFloat': [[ct.c_int64, ct.POINTER(ct.c_float)]],
            'kvScriptEnvvarGetInt': [[ct.c_int64, ct.POINTER(ct.c_int)]],
            'kvScriptEnvvarOpen': [[ct.c_int, ct.c_char_p, ct.POINTER(ct.c_int), ct.POINTER(ct.c_int)], ct.c_int64],
            'kvScriptEnvvarSetData': [[ct.c_int64, ct.c_void_p, ct.c_int, ct.c_int]],
            'kvScriptEnvvarSetFloat': [[ct.c_int64, ct.c_float]],
            'kvScriptEnvvarSetInt': [[ct.c_int64, ct.c_int]],
            'kvScriptGetText': [[ct.c_int, ct.POINTER(ct.c_int), ct.POINTER(ct.c_ulong), ct.POINTER(ct.c_uint), ct.POINTER(ct.c_char), ct.c_size_t]],
            'kvScriptLoadFile': [[ct.c_int, ct.c_int, ct.c_char_p]],
            'kvScriptLoadFileOnDevice': [[ct.c_int, ct.c_int, ct.c_char_p]],
            'kvScriptRequestText': [[ct.c_int, ct.c_uint, ct.c_uint]],
            'kvScriptSendEvent': [[ct.c_int, ct.c_int, ct.c_int, ct.c_int, ct.c_uint]],
            'kvScriptStart': [[ct.c_int, ct.c_int]],
            'kvScriptStatus': [[ct.c_int, ct.c_int, ct.POINTER(ct.c_uint)]],
            'kvScriptStop': [[ct.c_int, ct.c_int, ct.c_int]],
            'kvScriptTxeGetData': [[ct.c_char_p, ct.c_int, ct.c_void_p, ct.POINTER(ct.c_uint)]],
            'kvScriptUnload': [[ct.c_int, ct.c_int]],
            'kvSetNotifyCallback': [[ct.c_int, KVCALLBACK_T, ct.c_void_p, ct.c_uint]],
        }

        def __init__(self, ct_dll):
            # set default values for function_prototypes
            self.default_restype = ct.c_int
            self.default_errcheck = self._error_check
            super(CanlibDll, self).__init__(ct_dll, **self.function_prototypes)

        def _error_check(self, result, func, arguments):
            """Error function used in ctype calls for canlib DLL."""
            if result < 0:
                raise can_error(result)
            else:
                return result